<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="22.86" y1="18.796" x2="58.908" y2="18.669" width="0" layer="20"/>
<wire x1="58.908" y1="18.669" x2="58.908" y2="50.343" width="0" layer="20"/>
<wire x1="58.908" y1="50.343" x2="22.86" y2="50.47" width="0" layer="20"/>
<wire x1="22.86" y1="50.47" x2="22.86" y2="18.796" width="0" layer="20"/>
</plain>
<libraries>
<library name="fab">
<packages>
<package name="C1206FAB">
</package>
<package name="LED1206FAB">
<description>LED1206 FAB style (smaller pads to allow trace between)</description>
</package>
<package name="SOT23">
<description>&lt;b&gt;SOT 23&lt;/b&gt;</description>
</package>
<package name="1X06SMD">
</package>
<package name="R1206FAB">
</package>
</packages>
</library>
<library name="RN4871-V_RM118">
<packages>
<package name="XCVR_RN4871-V/RM118">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="D1" library="fab" package="LED1206FAB" value="LED RED">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="fab" package="LED1206FAB" value="LED GREEN">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="fab" package="SOT23" value="3.3V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="fab" package="1X06SMD" value="TFDI 3.3V">
<attribute name="NAME"/>
</element>
<element name="R1" library="fab" package="R1206FAB" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="fab" package="R1206FAB" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="fab" package="R1206FAB" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="RN4871-V_RM118" package="XCVR_RN4871-V/RM118" value="RN4871-V">
<attribute name="AVAILABILITY" value="Unavailable"/>
<attribute name="DESCRIPTION" value=" Bluetooth 4.2 BLE Module Shielded Antenna ASCII Interface 9x11.5mm "/>
<attribute name="MF" value="Microchip"/>
<attribute name="MP" value="RN4871-V/RM118"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="SMD-16 Microchip"/>
<attribute name="PRICE" value="None"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="fab" package="C1206FAB" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U1" pad="2"/>
<contactref element="U1" pad="13"/>
<contactref element="IC1" pad="3"/>
<contactref element="J1" pad="1"/>
<contactref element="R2" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="J1" pad="3"/>
<contactref element="IC1" pad="2"/>
</signal>
<signal name="VCC3.3">
<contactref element="IC1" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="U1" pad="14"/>
<contactref element="D1" pad="1"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="RST">
<contactref element="R1" pad="1"/>
<contactref element="U1" pad="10"/>
</signal>
<signal name="FTDIRX">
<contactref element="U1" pad="7"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="FTDITX">
<contactref element="U1" pad="8"/>
<contactref element="J1" pad="5"/>
</signal>
<signal name="N$3">
<contactref element="D1" pad="2"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="D2" pad="2"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="U1" pad="12"/>
<contactref element="D2" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
